H36Q_005

10/02/03

ramp7 unrecorded good x,z,i/s
flow pH 5 buffer ~ 3 min at Fx = 20 pN
Record on minitweezers in pen file = pH5

ramp 5
a1 	high
a2
a3
missed recording
a4
a5
a6
a7
a8
a9	low
a10
a11
a12
a13
a14	switched to file B
hpping changed therefore flow more pH 5 buffer ~ 3 min utter but broke

ps1 	free bead (not AA or CT) forgot to unplug power supply
ps2	free bead after AA and CT