H36Q_006

10/02/03

ramp7 unrecorded good x,z,i/s
flow pH 5 buffer ~ 5 min at Fx = 10 - 20 pN
Record on minitweezers in pen file = pH5

ramp 5
a1 	

odd hopping b/c buffer not fully exchanged ???
flow phi 5 buffer again

ramp5  3-10,100,0
a2
a3
a4
a5
a6
a7
a8
a9	
a10
a11
a12
a13	switched to file B
a14	
a15
a16
a17
a18
a19
a20	stopped hopping???

ramp5 3-10,100,0 but forgot to unplug

100,000 Hz 1,000,000 points
ps1 	free bead (not AA or CT) 
ps2	free bead after AA and CT