H36Q_008

10/02/04

Power = 10,000
Gain = 1.25V
Channel 1 y-axis
50 kHz - 3,000,000 points

ramp 7 not recorded 
good x,z,i/s
change to pH 5
~ 3 min at 20 pN Fx

pH5 = minitweezer file

ramp 5 on minitweezers 3 - 10,100,0

a1	high
a2
a3
a4
a5
a6	low
a7
a8
a9
a10
a11
a12
a13
a14
a15	switched to file B
a16
a17
a18	high 	program froze ~ 10 sec during data collection
a19	mid low
a20	mid high
ramp 5 - high sampling resolution on laptop - forgot to unplug power supply ???

ps1	free bead at position of break 
ps2	free bead away from pipette tip
ps3	free bead after center trap and auto align

Stokes test = 3.14 um bead (3.18 expected)