H36Q_009

10/02/04

Power = 10,000
Gain = 1.25V
Channel 1 y-axis
50 kHz - 3,000,000 points

open minitweezer file = data
ramp 7 3-20,100,0
good x,z,i/s
change to pH 5
~ 3 min at 16 pN Fx

ramp 5 on minitweezers 3 - 10,100,0

a1	high	drift a problem
a2
a3	high
a4
a5	high
a6	
a7
a8	stopped hopping (??) pulled to higher force
a9	low
a10
a11
a12
a13	switched to file B
a14
a15	
a16
a17
a18	
a19	
a20	
a21
a22
a23
a24
a25	high
a26 	mid
a27 	mid low	switched to file C
a28 	lower
a29	mid high
a30	mid

ramp 5 - high sampling resolution on laptop - 3-10,100,0

ps1	free bead at position of break 
ps2	free bead away from pipette tip
ps3	free bead after center trap and auto align