H36Q_011

10/02/05

Power = 10,000
Gain = 1.25V
Channel 1 y-axis
50 kHz - 3,000,000 points

open minitweezer file = data
ramp 7 3-20,100,0 on laptop
good x,z,i/s
change to pH 5
~ 3 min at 20 pN Fx

ramp5_1 on laptop 3 - 10,100,0

a1	high	
a2
a3	
a4
a5	
a6	
a7
a8	
a9	(froze on mt)
a10	low

Problems saving data b/c laptop disk full
close minitweezers file while I tried to fix the issue
after about 30 minutes
flow pH 5 ~ 3 min at 15 pN Fx
open new minitweezers file = data2

a11	high
a12
a13	
a14	odd hopping behavior stopped in F state and started again
a15	
a16
a17
a18	
a19	
a20	
a21
a22	low	stopped hopping - picked up 2nd fiber ???

broke

ps1	free bead at position of break - forgot to unplug power supply
ps2	free bead away from pipette tip
ps3	free bead after center trap and auto align